{"text_format":"2","workbook":"xlsx","n_sheets":9,"sheets":["采样机控制站","车辆定位站","封装机控制站","智能刷卡站","逻辑控制站","数据库处理站","操作员站","采样日志","干湿分类识别站"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"采样机控制站","index":0,"n_rows":77,"n_cols":9,"rows_kept":77,"cut":false,"hidden":false,"merged":[[2,2,3,8]]}
[]
[]
[null,null,"采样机控制站"]
[]
[null,null,"IDL类型","点名",null,"数据类型","说明","数据源","类型"]
[null,null,"uint32","DomainID","域ID","OUInt32","域ID","配置库","配置"]
[null,null,"string","DomainName","域名","OString","域名","配置库","配置"]
[null,null,"uint8","SampleType","采样机类型(1:随机深度,2:全段面)","OInt32","采样机类型(1:随机深度,2:全段面)","PLC","Output"]
[null,null,"uint8","ControlType","远程控制状态(1:就地,2:远程)","OInt32","远程控制状态(1:就地,2:远程)","PLC","Output"]
[null,null,"uint8","StartSample","启动采样","OByte","启动采样","PLC","Output"]
[null,null,"uint8","StopSample","停止采样","OInt32","停止采样","PLC","Output"]
[null,null,"uint8","Reset","系统复位","OInt32","系统复位","PLC","Output"]
[null,null,"uint16","UnifiedDepth","统一深度(全段面采样时使用)","OInt32","统一深度(全段面采样时使用)","PLC","Output"]
[null,null,"uint8","SampleOrder","大车行进顺序(1:原点往外，2:往原点采)","OInt32","大车行进顺序(1:原点往外，2:往原点采)","PLC","Output"]
[null,null,"uint8","TotalPoints","采样点数量","OInt32","采样点数量","PLC","Output"]
[null,null,"uint16","X1","采样点1X","OInt32","采样点1X","PLC","Output"]
[null,null,"uint16","Y1","采样点1Y","OInt32","采样点1Y","PLC","Output"]
[null,null,"uint16","Z1","采样点1Z","OInt32","采样点1Z","PLC","Output"]
[null,null,"uint8","O1","采样点1落料选择(1:旁路,2:破碎机)","OInt32","采样点1落料选择(1:旁路,2:破碎机)","PLC","Output"]
[null,null,"uint16","X2","采样点2X","OInt32","采样点2X","PLC","Output"]
[null,null,"uint16","Y2","采样点2Y","OInt32","采样点2Y","PLC","Output"]
[null,null,"uint16","Z2","采样点2Z","OInt32","采样点2Z","PLC","Output"]
[null,null,"uint8","O2","采样点2落料选择(1:旁路,2:破碎机)","OInt32","采样点2落料选择(1:旁路,2:破碎机)","PLC","Output"]
[null,null,"uint16","X3","采样点3X","OInt32","采样点3X","PLC","Output"]
[null,null,"uint16","Y3","采样点3Y","OInt32","采样点3Y","PLC","Output"]
[null,null,"uint16","Z3","采样点3Z","OInt32","采样点3Z","PLC","Output"]
[null,null,"uint8","O3","采样点3落料选择(1:旁路,2:破碎机)","OInt32","采样点3落料选择(1:旁路,2:破碎机)","PLC","Output"]
[null,null,"uint16","X4","采样点4X","OInt32","采样点4X","PLC","Output"]
[null,null,"uint16","Y4","采样点4Y","OInt32","采样点4Y","PLC","Output"]
[null,null,"uint16","Z4","采样点4Z","OInt32","采样点4Z","PLC","Output"]
[null,null,"uint8","O4","采样点4落料选择(1:旁路,2:破碎机)","OInt32","采样点4落料选择(1:旁路,2:破碎机)","PLC","Output"]
[null,null,"uint16","X5","采样点5X","OInt32","采样点5X","PLC","Output"]
[null,null,"uint16","Y5","采样点5Y","OInt32","采样点5Y","PLC","Output"]
[null,null,"uint16","Z5","采样点5Z","OInt32","采样点5Z","PLC","Output"]
[null,null,"uint8","O5","采样点5落料选择(1:旁路,2:破碎机)","OInt32","采样点5落料选择(1:旁路,2:破碎机)","PLC","Output"]
[null,null,"uint16","X6","采样点6X","OInt32","采样点6X","PLC","Output"]
[null,null,"uint16","Y6","采样点6Y","OInt32","采样点6Y","PLC","Output"]
[null,null,"uint16","Z6","采样点6Z","OInt32","采样点6Z","PLC","Output"]
[null,null,"uint8","O6","采样点6落料选择(1:旁路,2:破碎机)","OInt32","采样点6落料选择(1:旁路,2:破碎机)","PLC","Output"]
[null,null,"uint8","PositionCheck","位置确认，开始下降","OByte","位置确认，开始下降","PLC","Output"]
[null,null,"uint8","Command","采样命令","OInt32","采样命令","PLC","Output"]
[null,null,"uint8","BackState"," 采样状态返回","OInt32"," 采样状态返回","PLC","Output"]
[null,null,"uint8","EmergencyUp","紧急提升","OInt32","紧急提升","PLC","Output"]
[null,null,"uint8","EmergencyStop","系统急停","OInt32","系统急停","PLC","Output"]
[null,null,"uint8","StartBelt1","启动皮带1","OInt32","启动皮带1","PLC","Output"]
[null,null,"uint8","StopBelt1","关闭皮带1","OInt32","关闭皮带1","PLC","Output"]
[null,null,"uint8","StartCrush1","启动破碎机1","OInt32","启动破碎机1","PLC","Output"]
[null,null,"uint8","StopCrush1","关闭破碎机1","OInt32","关闭破碎机1","PLC","Output"]
[null,null,"uint8","StartBelt2","启动皮带2","OInt32","启动皮带2","PLC","Output"]
[null,null,"uint8","StopBelt2","关闭皮带2","OInt32","关闭皮带2","PLC","Output"]
[null,null,"uint8","StartCrush2","启动破碎机2","OInt32","启动破碎机2","PLC","Output"]
[null,null,"uint8","StopCrush2","关闭破碎机2","OInt32","关闭破碎机2","PLC","Output"]
[null,null,"uint8","StartDivider","启动缩分器","OInt32","启动缩分器","PLC","Output"]
[null,null,"uint8","StopDivider","关闭缩分器","OInt32","关闭缩分器","PLC","Output"]
[null,null,"uint16","ReductionRatio","缩分比","OInt33","缩分比","PLC","Output"]
[null,null,"uint8","StartCoalDistributor","打开布煤器","OInt34","打开布煤器","PLC","Output"]
[null,null,"uint8","StopCoalDistributor","关闭布煤器","OInt35","关闭布煤器","PLC","Output"]
[]
[null,null,"uint16","BigPoint","大车位置","OInt32","大车位置","PLC","Input"]
[null,null,"uint16","SmallPoint","小车位置","OInt32","小车位置","PLC","Input"]
[null,null,"uint16","DepthPoint","深度位置","OInt32","深度位置","PLC","Input"]
[null,null,"uint8","HasToXY","已经到达坐标点","OByte","已经到达坐标点","PLC","Input"]
[null,null,"uint8","HasSamplePoints","已采样点数","OInt32","已采样点数","PLC","Input"]
[null,null,"uint8","GameOver","采样完成","OInt32","采样完成","PLC","Input"]
[null,null,"uint16","BackState"," 采样状态返回","OInt32"," 采样状态返回","PLC","Input"]
[null,null,"uint8","SampleState","采样机状态","OInt32","采样机状态","PLC","Input"]
[null,null,"uint8","Belt1State","皮带1状态","OInt32","皮带1状态","PLC","Input"]
[null,null,"uint8","Belt2State","皮带2状态","OInt32","皮带2状态","PLC","Input"]
[null,null,"uint8","Crush1State","破碎机1状态","OInt32","破碎机1状态","PLC","Input"]
[null,null,"uint8","Crush2State","破碎机2状态","OInt32","破碎机2状态","PLC","Input"]
[null,null,"uint8","DividerState","缩分器状态","OInt32","缩分器状态","PLC","Input"]
[null,null,"uint8","BigLimit","大车驶出限位","Obyte","大车驶出限位","PLC","Input"]
[null,null,"uint8","BigZeroLimit","大车零点限位","Obyte","大车零点限位","PLC","Input"]
[null,null,"uint8","SmallLimit","小车驶出限位","Obyte","小车驶出限位","PLC","Input"]
[null,null,"uint8","SmallZeroLimit","小车零点限位","Obyte","小车零点限位","PLC","Input"]
[null,null,"uint8","UpLimit","升降高限位","Obyte","升降高限位","PLC","Input"]
[null,null,"uint8","DownLimit","升降低限位","Obyte","升降低限位","PLC","Input"]

{"sheet":"车辆定位站","index":1,"n_rows":46,"n_cols":7,"rows_kept":46,"cut":false,"hidden":false,"merged":[[2,1,4,1],[5,1,44,1],[2,2,3,6]]}
[]
[]
[null,null,"车辆定位站"]
[]
[null,null,"点名","数据类型","说明","数据源","类型"]
[null,"输出信号","DomainID","OUInt32","域ID",null,"配置"]
[null,null,"DomainName","OString","域名",null,"配置"]
[null,null,"X","OInt32","安装位置X","配置信息"]
[null,null,"Y","OInt32","安装位置Y","配置信息"]
[null,null,"Z","OInt32","安装离地高度","配置信息"]
[null,null,"DLeftTopX","OByte","限制区左上角X","配置信息"]
[null,null,"DLeftTopY","OInt32","限制区左上角Y","配置信息"]
[null,null,"DRightBottomX","OByte","限制区右下角X","配置信息"]
[null,null,"DRightBottomY","OInt32","限制区右下角Y","配置信息"]
[null,null,"RLeftTopX","OByte","识别区左上角X","Output"]
[null,null,"RLeftTopY","OInt32","识别区左上角Y","Output"]
[null,null,"RRightBottomX","OByte","识别区右下角X","Output"]
[null,null,"RRightBottomY","OInt32","识别区右下角Y","Output"]
[null,null,"CloudPoints","Bytes","点云数据","Output"]
[null,null,"SampleOrder","OInt32","大车行进顺序(1:原点往外，2:往原点采)","Input"]
[null,null,"TotalPoints","OInt32","采样点数量","Input"]
[null,null,"X1","OInt32","采样点1X","Output"]
[null,null,"Y1","OInt32","采样点1Y","Output"]
[null,null,"Z1","OInt32","采样点1Z","Output"]
[null,null,"O1","OInt32","采样点1落料选择(1:旁路,2:破碎机)","Input"]
[null,null,"X2","OInt32","采样点2X","Output"]
[null,null,"Y2","OInt32","采样点2Y","Output"]
[null,null,"Z2","OInt32","采样点2Z","Output"]
[null,null,"O2","OInt32","采样点2落料选择(1:旁路,2:破碎机)","Input"]
[null,null,"X3","OInt32","采样点3X","Output"]
[null,null,"Y3","OInt32","采样点3Y","Output"]
[null,null,"Z3","OInt32","采样点3Z","Output"]
[null,null,"O3","OInt32","采样点3落料选择(1:旁路,2:破碎机)","Input"]
[null,null,"X4","OInt32","采样点4X","Output"]
[null,null,"Y4","OInt32","采样点4Y","Output"]
[null,null,"Z4","OInt32","采样点4Z","Output"]
[null,null,"O4","OInt32","采样点4落料选择(1:旁路,2:破碎机)","Input"]
[null,null,"X5","OInt32","采样点5X","Output"]
[null,null,"Y5","OInt32","采样点5Y","Output"]
[null,null,"Z5","OInt32","采样点5Z","Output"]
[null,null,"O5","OInt32","采样点5落料选择(1:旁路,2:破碎机)","Input"]
[null,null,"X6","OInt32","采样点6X","Output"]
[null,null,"Y6","OInt32","采样点6Y","Output"]
[null,null,"Z6","OInt32","采样点6Z","Output"]
[null,null,"O6","OInt32","采样点6落料选择(1:旁路,2:破碎机)","Input"]
[null,null,"BeginCalculate","OInt33","开始计算生成点位","Input"]

{"sheet":"封装机控制站","index":2,"n_rows":16,"n_cols":6,"rows_kept":16,"cut":false,"hidden":false,"merged":[[2,1,3,5]]}
[]
[]
[null,"封装机控制站"]
[]
[null,"点名","数据类型","说明","数据源","类型"]
[null,"DomainID","OUInt32","域ID",null,"配置"]
[null,"DomainName","OString","域名",null,"配置"]
[null,"ControlType","OInt32","远程控制状态(1:就地,2:远程)","手动/自动"]
[null,"Parameter","OInt32","命令参数"]
[null,"Command","OInt32","命令号"]
[null,"BackParam","OByte","命令返回参数"]
[null,"CommandBack","OInt32","命令返回"]
[null,"State","OInt32","设备状态"]
[null,"Warning","OInt32","设备故障"]
[null,"Speed","OInt32","电机转速"]
[null,"Reset","OInt32","复位"]

{"sheet":"智能刷卡站","index":3,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[[2,1,3,5]]}
[]
[]
[null,"智能刷卡机"]
[]
[null,"点名","数据类型","说明","数据源","类型"]
[null,"DomainID","OUInt32","域ID",null,"配置"]
[null,"DomainName","OString","域名",null,"配置"]
[null,"RFID","OString","卡号","Output","Output"]
[null,"Waring","OString","提示信息","Input","Input"]
[null,"Voice","OInt32","语音编号","Input","Input"]
[null,"TakeOut1","OInt32","发卡1",null,"Input"]
[null,"Code1","OString","编码卡号1",null,"Output"]
[null,"TakeOutOver1","OInt32","发卡完成1",null,"Output"]
[null,"TakeOut2","OInt32","发卡2",null,"Input"]
[null,"Code2","OString","编码卡号2",null,"Output"]
[null,"TakeOutOver2","OInt32","发卡完成2",null,"Output"]
[null,"CarNumber","OString","车牌号"]

{"sheet":"逻辑控制站","index":4,"n_rows":47,"n_cols":7,"rows_kept":47,"cut":false,"hidden":false,"merged":[[2,1,4,1],[5,1,45,1],[2,2,3,6]]}
[]
[]
[null,null,"逻辑控制站"]
[]
[null,null,"点名","数据类型","说明","数据源","类型"]
[null,"输出信号","DomainID","OUInt32","域ID",null,"配置"]
[null,null,"DomainName","OString","域名",null,"配置"]
[null,null,"AllowSample","OInt32","是否自动采样(1:自动启动，2:人工启动)",null,"配置"]
[null,null,"RFID","OString","卡号",null,"Input"]
[null,null,"Y","OInt32","安装位置Y",null,"配置信息"]
[null,null,"Z","OInt32","安装离地高度",null,"配置信息"]
[null,null,"DLeftTopX","OByte","限制区左上角X",null,"配置信息"]
[null,null,"DLeftTopY","OInt32","限制区左上角Y",null,"配置信息"]
[null,null,"DRightBottomX","OByte","限制区右下角X",null,"配置信息"]
[null,null,"DRightBottomY","OInt32","限制区右下角Y",null,"配置信息"]
[null,null,"RLeftTopX","OByte","识别区左上角X",null,"Output"]
[null,null,"RLeftTopY","OInt32","识别区左上角Y",null,"Output"]
[null,null,"RRightBottomX","OByte","识别区右下角X",null,"Output"]
[null,null,"RRightBottomY","OInt32","识别区右下角Y",null,"Output"]
[null,null,"CloudPoints","Bytes","点云数据",null,"Output"]
[null,null,"SampleOrder","OInt32","大车行进顺序(1:原点往外，2:往原点采)",null,"Input"]
[null,null,"TotalPoints","OInt32","采样点数量",null,"Input"]
[null,null,"X1","OInt32","采样点1X",null,"Output"]
[null,null,"Y1","OInt32","采样点1Y",null,"Output"]
[null,null,"Z1","OInt32","采样点1Z",null,"Output"]
[null,null,"O1","OInt32","采样点1落料选择(1:旁路,2:破碎机)",null,"Input"]
[null,null,"X2","OInt32","采样点2X",null,"Output"]
[null,null,"Y2","OInt32","采样点2Y",null,"Output"]
[null,null,"Z2","OInt32","采样点2Z",null,"Output"]
[null,null,"O2","OInt32","采样点2落料选择(1:旁路,2:破碎机)",null,"Input"]
[null,null,"X3","OInt32","采样点3X",null,"Output"]
[null,null,"Y3","OInt32","采样点3Y",null,"Output"]
[null,null,"Z3","OInt32","采样点3Z",null,"Output"]
[null,null,"O3","OInt32","采样点3落料选择(1:旁路,2:破碎机)",null,"Input"]
[null,null,"X4","OInt32","采样点4X",null,"Output"]
[null,null,"Y4","OInt32","采样点4Y",null,"Output"]
[null,null,"Z4","OInt32","采样点4Z",null,"Output"]
[null,null,"O4","OInt32","采样点4落料选择(1:旁路,2:破碎机)",null,"Input"]
[null,null,"X5","OInt32","采样点5X",null,"Output"]
[null,null,"Y5","OInt32","采样点5Y",null,"Output"]
[null,null,"Z5","OInt32","采样点5Z",null,"Output"]
[null,null,"O5","OInt32","采样点5落料选择(1:旁路,2:破碎机)",null,"Input"]
[null,null,"X6","OInt32","采样点6X",null,"Output"]
[null,null,"Y6","OInt32","采样点6Y",null,"Output"]
[null,null,"Z6","OInt32","采样点6Z",null,"Output"]
[null,null,"O6","OInt32","采样点6落料选择(1:旁路,2:破碎机)",null,"Input"]
[null,null,"BeginCalculate","OInt33","开始计算生成点位",null,"Input"]

{"sheet":"数据库处理站","index":5,"n_rows":73,"n_cols":6,"rows_kept":73,"cut":false,"hidden":false,"merged":[[2,1,3,5]]}
[]
[]
[null,"数据库处理站"]
[]
[null,"点名","数据类型","说明","数据源","类型"]
[null,"DomainID","OUInt32","域ID",null,"配置"]
[null,"DomainName","OString","域名",null,"配置"]
[null,"RFID","OString","卡号","智能刷卡站","Input"]
[null,"AllowSampling","OInt32","允许采样",null,"Output"]
[null,"CarNumber","OString","车牌号",null,"Output"]
[null,"SamplePoint","OByte","采样点数",null,"Output"]
[null,"CarLength","OInt32","车厢长度",null,"Output"]
[null,"CarWidth","OInt32","车厢宽度",null,"Output"]
[null,"CarUp","OInt32","车厢高度",null,"Output"]
[null,"CarDown","OInt32","底盘高度",null,"Output"]
[null,"StepCount","OInt32","拉筋数",null,"Output"]
[null,"Step1","OInt32","拉筋1位置",null,"Output"]
[null,"Step2","OInt32","拉筋2位置",null,"Output"]
[null,"Step3","OInt32","拉筋3位置",null,"Output"]
[null,"Step4","OInt32","拉筋4位置",null,"Output"]
[null,"Step5","OInt32","拉筋5位置",null,"Output"]
[null,"MainCount","OInt32","破碎数量",null,"Output"]
[null,"BypassCount","OInt32","旁路数量",null,"Output"]
[null,"Waring","OString","提示信息",null,"Output"]
[null,"Voice","OInt32","语音编号",null,"Output"]
[null,"Code1","OString","编码卡号1","智能刷卡站","Input"]
[null,"TakeOutOver1","OInt32","发卡完成1","智能刷卡站","Input"]
[null,"Code2","OString","编码卡号2","智能刷卡站","Input"]
[null,"TakeOutOver2","OInt32","发卡完成2","智能刷卡站","Input"]
[null,"GameOver","OInt32","采样完成信号","采样机控制站","Input"]
[null,"TotalPoints","OInt32","采样点数量","采样机控制站","Input"]
[null,"Src-X1","OInt32","采样点1X","采样机控制站","Input"]
[null,"Src-Y1","OInt32","采样点1Y","采样机控制站","Input"]
[null,"Src-Z1","OInt32","采样点1Z","采样机控制站","Input"]
[null,"Src-O1","OInt32","采样点1落料口","采样机控制站","Input"]
[null,"Src-X2","OInt32","采样点2X","采样机控制站","Input"]
[null,"Src-Y2","OInt32","采样点2Y","采样机控制站","Input"]
[null,"Src-Z2","OInt32","采样点2Z","采样机控制站","Input"]
[null,"Src-O2","OInt32","采样点2落料口","采样机控制站","Input"]
[null,"Src-X3","OInt32","采样点3X","采样机控制站","Input"]
[null,"Src-Y3","OInt32","采样点3Y","采样机控制站","Input"]
[null,"Src-Z3","OInt32","采样点3Z","采样机控制站","Input"]
[null,"Src-O3","OInt32","采样点3落料口","采样机控制站","Input"]
[null,"Src-X4","OInt32","采样点4X","采样机控制站","Input"]
[null,"Src-Y4","OInt32","采样点4Y","采样机控制站","Input"]
[null,"Src-Z4","OInt32","采样点4Z","采样机控制站","Input"]
[null,"Src-O4","OInt32","采样点4落料口","采样机控制站","Input"]
[null,"Src-X5","OInt32","采样点5X","采样机控制站","Input"]
[null,"Src-Y5","OInt32","采样点5Y","采样机控制站","Input"]
[null,"Src-Z5","OInt32","采样点5Z","采样机控制站","Input"]
[null,"Src-O5","OInt32","采样点5落料口","采样机控制站","Input"]
[null,"Src-X6","OInt32","采样点6X","采样机控制站","Input"]
[null,"Src-Y6","OInt32","采样点6Y","采样机控制站","Input"]
[null,"Src-Z6","OInt32","采样点6Z","采样机控制站","Input"]
[null,"Src-O6","OInt32","采样点6落料口","采样机控制站","Input"]
[null,"Real-X1","OInt32","实际采样点1X","采样机控制站","Input"]
[null,"Real-Y1","OInt32","实际采样点1Y","采样机控制站","Input"]
[null,"Real-Z1","OInt32","实际采样点1Z","采样机控制站","Input"]
[null,"Real-X2","OInt32","实际采样点2X","采样机控制站","Input"]
[null,"Real-Y2","OInt32","实际采样点2Y","采样机控制站","Input"]
[null,"Real-Z2","OInt32","实际采样点2Z","采样机控制站","Input"]
[null,"Real-X3","OInt32","实际采样点3X","采样机控制站","Input"]
[null,"Real-Y3","OInt32","实际采样点3Y","采样机控制站","Input"]
[null,"Real-Z3","OInt32","实际采样点3Z","采样机控制站","Input"]
[null,"Real-X4","OInt32","实际采样点4X","采样机控制站","Input"]
[null,"Real-Y4","OInt32","实际采样点4Y","采样机控制站","Input"]
[null,"Real-Z4","OInt32","实际采样点4Z","采样机控制站","Input"]
[null,"Real-X5","OInt32","实际采样点5X","采样机控制站","Input"]
[null,"Real-Y5","OInt32","实际采样点5Y","采样机控制站","Input"]
[null,"Real-Z5","OInt32","实际采样点5Z","采样机控制站","Input"]
[null,"Real-X6","OInt32","实际采样点6X","采样机控制站","Input"]
[null,"Real-Y6","OInt32","实际采样点6Y","采样机控制站","Input"]
[null,"Real-Z6","OInt32","实际采样点6Z","采样机控制站","Input"]

{"sheet":"操作员站","index":6,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"采样日志","index":7,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"干湿分类识别站","index":8,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}